(export (version "E")
  (design
    (source "I:\\Proyectos\\numPAD\\numPAD_MCU\\numPAD_MCU.kicad_sch")
    (date "08/03/2022 14:58:14")
    (tool "Eeschema (6.0.2)")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "numPAD_MCU.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "J1")
      (value "Conn_01x06")
      (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical")
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "8c077155-3d1b-4c61-8ad6-aa7da49ff67a"))
    (comp (ref "J2")
      (value "Conn_01x06")
      (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical")
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "abc425ae-34db-440c-baf2-199506429483"))
    (comp (ref "U1")
      (value "ARDUINO_MICRO_SHIELD")
      (footprint "Creadas:ARDUINO_MICRO_SHIELD")
      (libsource (lib "Creadas") (part "ARDUINO_MICRO_SHIELD") (description "Arduino Micro shield"))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "37c25398-65cf-4ddd-a150-430f469ed645")))
  (libparts
    (libpart (lib "Connector_Generic") (part "Conn_01x06")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x06")
        (field (name "Datasheet") "~"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))))
    (libpart (lib "Creadas") (part "ARDUINO_MICRO_SHIELD")
      (description "Arduino Micro shield")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "ARDUINO_MICRO_SHIELD"))
      (pins
        (pin (num "2") (name "2/SDA") (type "bidirectional"))
        (pin (num "3") (name "3(PWM)/SCL") (type "bidirectional"))
        (pin (num "3.3V") (name "3.3V") (type "power_in"))
        (pin (num "4") (name "4/A6") (type "bidirectional"))
        (pin (num "5") (name "5(PWM)") (type "bidirectional"))
        (pin (num "5V") (name "+5V") (type "power_in"))
        (pin (num "6") (name "6(PWM)/A7") (type "bidirectional"))
        (pin (num "7") (name "7") (type "bidirectional"))
        (pin (num "8") (name "8/A8") (type "bidirectional"))
        (pin (num "9") (name "9(PWM)/A9") (type "bidirectional"))
        (pin (num "10") (name "10(PWM)/A10") (type "bidirectional"))
        (pin (num "11") (name "11(PWM)") (type "bidirectional"))
        (pin (num "12") (name "12/A11") (type "bidirectional"))
        (pin (num "13") (name "13(PWM)") (type "bidirectional"))
        (pin (num "A0") (name "A0") (type "bidirectional"))
        (pin (num "A1") (name "A1") (type "bidirectional"))
        (pin (num "A2") (name "A2") (type "bidirectional"))
        (pin (num "A3") (name "A3") (type "bidirectional"))
        (pin (num "A4") (name "A4") (type "bidirectional"))
        (pin (num "A5") (name "A5") (type "bidirectional"))
        (pin (num "AREF") (name "AREF") (type "power_in"))
        (pin (num "GND") (name "GND") (type "power_in"))
        (pin (num "MI") (name "MISO") (type "bidirectional"))
        (pin (num "MO") (name "MOSI") (type "bidirectional"))
        (pin (num "NC") (name "") (type "no_connect"))
        (pin (num "RST") (name "RESET") (type "bidirectional"))
        (pin (num "RX") (name "0/RX") (type "bidirectional"))
        (pin (num "SCK") (name "SCK") (type "bidirectional"))
        (pin (num "SS") (name "RX_LED/SS") (type "bidirectional"))
        (pin (num "TX") (name "1/TX") (type "bidirectional"))
        (pin (num "VI") (name "VIN") (type "power_in")))))
  (libraries
    (library (logical "Connector_Generic")
      (uri "C:\\Program Files\\KiCad\\6.0\\share\\kicad\\symbols\\/Connector_Generic.kicad_sym"))
    (library (logical "Creadas")
      (uri "C:/Users/atanc/Documents/KiCad/6.0/symbols/Creadas.kicad_sym")))
  (nets
    (net (code "1") (name "Net-(J1-Pad1)")
      (node (ref "J1") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U1") (pin "A4") (pinfunction "A4") (pintype "bidirectional")))
    (net (code "2") (name "Net-(J1-Pad2)")
      (node (ref "J1") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U1") (pin "A3") (pinfunction "A3") (pintype "bidirectional")))
    (net (code "3") (name "Net-(J1-Pad3)")
      (node (ref "J1") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U1") (pin "A2") (pinfunction "A2") (pintype "bidirectional")))
    (net (code "4") (name "Net-(J1-Pad4)")
      (node (ref "J1") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "A1") (pinfunction "A1") (pintype "bidirectional")))
    (net (code "5") (name "Net-(J1-Pad5)")
      (node (ref "J1") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U1") (pin "A0") (pinfunction "A0") (pintype "bidirectional")))
    (net (code "6") (name "Net-(J1-Pad6)")
      (node (ref "J1") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U1") (pin "5V") (pinfunction "+5V") (pintype "power_in")))
    (net (code "7") (name "Net-(J2-Pad1)")
      (node (ref "J2") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U1") (pin "6") (pinfunction "6(PWM)/A7") (pintype "bidirectional")))
    (net (code "8") (name "Net-(J2-Pad2)")
      (node (ref "J2") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U1") (pin "5") (pinfunction "5(PWM)") (pintype "bidirectional")))
    (net (code "9") (name "Net-(J2-Pad3)")
      (node (ref "J2") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U1") (pin "4") (pinfunction "4/A6") (pintype "bidirectional")))
    (net (code "10") (name "Net-(J2-Pad4)")
      (node (ref "J2") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "3") (pinfunction "3(PWM)/SCL") (pintype "bidirectional")))
    (net (code "11") (name "Net-(J2-Pad5)")
      (node (ref "J2") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U1") (pin "2") (pinfunction "2/SDA") (pintype "bidirectional")))
    (net (code "12") (name "Net-(J2-Pad6)")
      (node (ref "J2") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U1") (pin "GND") (pinfunction "GND") (pintype "power_in")))
    (net (code "13") (name "unconnected-(U1-Pad3.3V)")
      (node (ref "U1") (pin "3.3V") (pinfunction "3.3V") (pintype "power_in+no_connect")))
    (net (code "14") (name "unconnected-(U1-Pad7)")
      (node (ref "U1") (pin "7") (pinfunction "7") (pintype "bidirectional+no_connect")))
    (net (code "15") (name "unconnected-(U1-Pad8)")
      (node (ref "U1") (pin "8") (pinfunction "8/A8") (pintype "bidirectional+no_connect")))
    (net (code "16") (name "unconnected-(U1-Pad9)")
      (node (ref "U1") (pin "9") (pinfunction "9(PWM)/A9") (pintype "bidirectional+no_connect")))
    (net (code "17") (name "unconnected-(U1-Pad10)")
      (node (ref "U1") (pin "10") (pinfunction "10(PWM)/A10") (pintype "bidirectional+no_connect")))
    (net (code "18") (name "unconnected-(U1-Pad11)")
      (node (ref "U1") (pin "11") (pinfunction "11(PWM)") (pintype "bidirectional+no_connect")))
    (net (code "19") (name "unconnected-(U1-Pad12)")
      (node (ref "U1") (pin "12") (pinfunction "12/A11") (pintype "bidirectional+no_connect")))
    (net (code "20") (name "unconnected-(U1-Pad13)")
      (node (ref "U1") (pin "13") (pinfunction "13(PWM)") (pintype "bidirectional+no_connect")))
    (net (code "21") (name "unconnected-(U1-PadA5)")
      (node (ref "U1") (pin "A5") (pinfunction "A5") (pintype "bidirectional+no_connect")))
    (net (code "22") (name "unconnected-(U1-PadAREF)")
      (node (ref "U1") (pin "AREF") (pinfunction "AREF") (pintype "power_in+no_connect")))
    (net (code "23") (name "unconnected-(U1-PadGND)")
      (node (ref "U1") (pin "GND") (pinfunction "GND") (pintype "power_in+no_connect")))
    (net (code "24") (name "unconnected-(U1-PadMI)")
      (node (ref "U1") (pin "MI") (pinfunction "MISO") (pintype "bidirectional+no_connect")))
    (net (code "25") (name "unconnected-(U1-PadMO)")
      (node (ref "U1") (pin "MO") (pinfunction "MOSI") (pintype "bidirectional+no_connect")))
    (net (code "26") (name "unconnected-(U1-PadNC)")
      (node (ref "U1") (pin "NC") (pintype "no_connect")))
    (net (code "27") (name "unconnected-(U1-PadNC)_1")
      (node (ref "U1") (pin "NC") (pintype "no_connect")))
    (net (code "28") (name "unconnected-(U1-PadRST)")
      (node (ref "U1") (pin "RST") (pinfunction "RESET") (pintype "bidirectional+no_connect")))
    (net (code "29") (name "unconnected-(U1-PadRST)_1")
      (node (ref "U1") (pin "RST") (pinfunction "RESET") (pintype "bidirectional+no_connect")))
    (net (code "30") (name "unconnected-(U1-PadRX)")
      (node (ref "U1") (pin "RX") (pinfunction "0/RX") (pintype "bidirectional+no_connect")))
    (net (code "31") (name "unconnected-(U1-PadSCK)")
      (node (ref "U1") (pin "SCK") (pinfunction "SCK") (pintype "bidirectional+no_connect")))
    (net (code "32") (name "unconnected-(U1-PadSS)")
      (node (ref "U1") (pin "SS") (pinfunction "RX_LED/SS") (pintype "bidirectional+no_connect")))
    (net (code "33") (name "unconnected-(U1-PadTX)")
      (node (ref "U1") (pin "TX") (pinfunction "1/TX") (pintype "bidirectional+no_connect")))
    (net (code "34") (name "unconnected-(U1-PadVI)")
      (node (ref "U1") (pin "VI") (pinfunction "VIN") (pintype "power_in+no_connect")))))