(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers")
    )
  )

  (net 0 "")
  (net 1 "Net-(J2-Pad5)")
  (net 2 "Net-(J2-Pad4)")
  (net 3 "unconnected-(U1-Pad3.3V)")
  (net 4 "Net-(J2-Pad3)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "unconnected-(U1-Pad7)")
  (net 9 "unconnected-(U1-Pad8)")
  (net 10 "unconnected-(U1-Pad9)")
  (net 11 "unconnected-(U1-Pad10)")
  (net 12 "unconnected-(U1-Pad11)")
  (net 13 "unconnected-(U1-Pad12)")
  (net 14 "unconnected-(U1-Pad13)")
  (net 15 "Net-(J1-Pad5)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad2)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "unconnected-(U1-PadA5)")
  (net 21 "unconnected-(U1-PadAREF)")
  (net 22 "Net-(U1-PadGND)")
  (net 23 "unconnected-(U1-PadMI)")
  (net 24 "unconnected-(U1-PadMO)")
  (net 25 "unconnected-(U1-PadNC)")
  (net 26 "unconnected-(U1-PadRST)")
  (net 27 "unconnected-(U1-PadRX)")
  (net 28 "unconnected-(U1-PadSCK)")
  (net 29 "unconnected-(U1-PadSS)")
  (net 30 "unconnected-(U1-PadTX)")
  (net 31 "unconnected-(U1-PadVI)")

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 6227A509) (tstamp 386a0090-0a46-4bfb-96d1-b3d435c60ba8)
    (at 123.2 76.5 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/abc425ae-34db-440c-baf2-199506429483")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.33 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b0c5723f-3e32-4297-b270-9ec72d96287f)
    )
    (fp_text value "Conn_01x06" (at -2.5 -2.7 180) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3438dc41-962e-4989-a941-ede9a05290f1)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a77f222a-7823-46b1-8e3a-d2a424b8632b)
    )
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 6632d75c-5002-438f-9c39-2c0837a9461c))
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 7431ff9e-72b1-43ae-bc6a-a31b80516d6e))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp 80a90ec1-2aa8-4ed8-ad49-eac8c1a98713))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp 8cc9ae96-0b56-4dcf-a834-c235f5443d6e))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 8e9fa413-942b-4c93-ae63-0c4810c88678))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp a7262880-7db7-4327-af28-4ff7a323ea6f))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 54c27061-0469-4ab6-bb4c-048a1ba1c9c9))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 6336394d-7e46-45c7-b073-13cf1cd71142))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp a90fe392-ecf6-4078-bb71-4cea6a1b7bf1))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp c6d4813c-be0f-4ef2-854c-de499e07b7b9))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 0007e6f5-ad9a-4848-9892-60b937c244a1))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 076a2071-392b-4454-8bc1-b0bf7fb5c914))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp 7f3f4807-4744-448d-971c-11cf29b1668e))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp e2631437-99d2-41f3-ba09-28f2b097e746))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp ed9081a8-9b09-40a3-a6e1-aa91cb2ab6d6))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 68df789b-75eb-4c44-92bb-64cefd789ca7))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 28664fad-ee1c-4d2d-80fd-4a23c02f9ccc))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp c72d815d-9c53-4baf-a58b-2bb3597edaf1))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 333c653a-0b05-4693-9635-b158ec4ad8d6))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 49bdaa67-149f-4f2e-8c60-9195ba6be32f))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-PadGND)") (pinfunction "Pin_6") (pintype "passive") (tstamp 74097e6c-0dc1-43ce-ab88-c08de32f66ac))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Creadas:ARDUINO_MICRO_SHIELD" (layer "B.Cu")
    (tedit 6227A5E7) (tstamp 5100842c-3667-440b-ab36-56657f94bcf2)
    (at 137.5875 121.4155 90)
    (tags "ARDUINO, MICRO")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/37c25398-65cf-4ddd-a150-430f469ed645")
    (attr through_hole)
    (fp_text reference "U1" (at 26.67 10.16 90) (layer "B.SilkS")
      (effects (font (size 1.7 1.7) (thickness 0.15)) (justify mirror))
      (tstamp 5c3b0cf4-ded2-406f-9482-b45e5017a66e)
    )
    (fp_text value "ARDUINO_MICRO_SHIELD" (at 26.67 7.62 90) (layer "B.SilkS")
      (effects (font (size 1.7 1.7) (thickness 0.15)) (justify mirror))
      (tstamp cff3cb6d-0ecc-4073-a57c-9876e1369344)
    )
    (fp_text user "USB" (at 46.99 8.89) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4982cb91-53ba-473c-b939-a87eccbf750d)
    )
    (fp_line (start 0 18) (end 48 18) (layer "B.SilkS") (width 0.15) (tstamp 31c0f056-ed58-4239-a02b-c761bc4e514a))
    (fp_line (start 45.212 11.43) (end 48.006 11.43) (layer "B.SilkS") (width 0.15) (tstamp 4df229c7-d077-40ba-827a-fab1f6604385))
    (fp_line (start 48 0) (end 0 0) (layer "B.SilkS") (width 0.15) (tstamp 63a482a8-7189-4ebd-8864-ff7696b71546))
    (fp_line (start 0 0) (end 0 18) (layer "B.SilkS") (width 0.15) (tstamp 9e282c7f-2222-4f8e-953f-5a0ece602fd6))
    (fp_line (start 45.212 6.35) (end 45.212 11.43) (layer "B.SilkS") (width 0.15) (tstamp c21c1a6c-c93a-40eb-bad8-c91faeab799f))
    (fp_line (start 48 18) (end 48 0) (layer "B.SilkS") (width 0.15) (tstamp c4601dc9-2740-4f2b-86b1-f1a709404201))
    (fp_line (start 48.006 6.35) (end 45.212 6.35) (layer "B.SilkS") (width 0.15) (tstamp ed5b326d-e5e4-43c7-a685-e8d87de527b2))
    (fp_circle (center 1 16.51) (end 1.5 16.51) (layer "B.SilkS") (width 0.15) (fill none) (tstamp 16fe967e-3023-49c9-8397-5ed83aa0513d))
    (fp_circle (center 1 1.254) (end 1.5 1.254) (layer "B.SilkS") (width 0.15) (fill none) (tstamp 210174ea-5887-4790-b6e2-4d3c76ff9da6))
    (fp_circle (center 47 1.254) (end 47.5 1.254) (layer "B.SilkS") (width 0.15) (fill none) (tstamp 51f94fe6-2135-4b7c-83d7-187b47b9f328))
    (fp_circle (center 47 16.51) (end 47.5 16.51) (layer "B.SilkS") (width 0.15) (fill none) (tstamp 9091a69e-f077-4408-8d8a-228725bb8650))
    (pad "2" thru_hole oval (at 44.14 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(U1-Pad12)") (pinfunction "12/A11") (pintype "bidirectional+no_connect") (tstamp 143c5a61-f991-4241-b3fc-28429d689230))
    (pad "2" thru_hole oval (at 18.74 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)") (pinfunction "2/SDA") (pintype "bidirectional") (tstamp 97a586f6-bfb4-4860-87c7-194f50d6be3d))
    (pad "3" thru_hole oval (at 21.28 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad4)") (pinfunction "3(PWM)/SCL") (pintype "bidirectional") (tstamp 2c01f2ab-8c6a-4735-90df-95c659622cc6))
    (pad "3.3V" thru_hole oval (at 41.6 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(U1-Pad3.3V)") (pinfunction "3.3V") (pintype "power_in+no_connect") (tstamp 360f49e7-fafb-4982-92b6-7fc4d1e4fd7e))
    (pad "4" thru_hole oval (at 23.82 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad3)") (pinfunction "4/A6") (pintype "bidirectional") (tstamp d1af22c5-bbc1-4456-9632-175ef268b4f6))
    (pad "5" thru_hole oval (at 26.36 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)") (pinfunction "5(PWM)") (pintype "bidirectional") (tstamp ae085b70-5f8c-410c-94db-c5c36bab6d4e))
    (pad "5V" thru_hole oval (at 16.2 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "+5V") (pintype "power_in") (tstamp 474e2b8c-f73d-49c0-80db-da5f32d468d2))
    (pad "6" thru_hole oval (at 28.9 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)") (pinfunction "6(PWM)/A7") (pintype "bidirectional") (tstamp 86699a8f-0312-4e4e-95e8-c89b7fbf13f8))
    (pad "7" thru_hole oval (at 31.44 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(U1-Pad7)") (pinfunction "7") (pintype "bidirectional+no_connect") (tstamp 07d32dd1-90dc-479c-90d8-2924798fe8d5))
    (pad "8" thru_hole oval (at 33.98 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(U1-Pad8)") (pinfunction "8/A8") (pintype "bidirectional+no_connect") (tstamp 6c1a57bf-6c9e-49fb-bbce-e3aed1d3b81b))
    (pad "9" thru_hole oval (at 36.52 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(U1-Pad9)") (pinfunction "9(PWM)/A9") (pintype "bidirectional+no_connect") (tstamp 072052ee-2d3d-47bb-a8c4-2f1bf63ec28e))
    (pad "10" thru_hole oval (at 39.06 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(U1-Pad10)") (pinfunction "10(PWM)/A10") (pintype "bidirectional+no_connect") (tstamp 833b3a8a-5308-478b-9efb-804dd58f7fd7))
    (pad "11" thru_hole oval (at 41.6 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(U1-Pad11)") (pinfunction "11(PWM)") (pintype "bidirectional+no_connect") (tstamp 66125229-c705-4ed3-95a2-13ba8cd9fdfe))
    (pad "13" thru_hole oval (at 44.14 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(U1-Pad13)") (pinfunction "13(PWM)") (pintype "bidirectional+no_connect") (tstamp ac5b15fa-b58e-44da-a575-0d5921d7437e))
    (pad "A0" thru_hole oval (at 36.52 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)") (pinfunction "A0") (pintype "bidirectional") (tstamp 9012aeee-cead-4a54-9744-ce0fb23536e6))
    (pad "A1" thru_hole oval (at 33.98 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)") (pinfunction "A1") (pintype "bidirectional") (tstamp ce1259f0-7c8b-4c03-8eae-6142d2535ddc))
    (pad "A2" thru_hole oval (at 31.44 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)") (pinfunction "A2") (pintype "bidirectional") (tstamp 096765f8-3ef4-4047-b785-8e943f9bc4f3))
    (pad "A3" thru_hole oval (at 28.9 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)") (pinfunction "A3") (pintype "bidirectional") (tstamp b15c4489-099e-4346-a866-2edc2840ce66))
    (pad "A4" thru_hole oval (at 26.36 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)") (pinfunction "A4") (pintype "bidirectional") (tstamp eda76021-7e32-4e6b-9e13-02caa8089fe6))
    (pad "A5" thru_hole oval (at 23.82 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-PadA5)") (pinfunction "A5") (pintype "bidirectional+no_connect") (tstamp 76285e48-7f1a-42d6-9127-0fb3fc56c01e))
    (pad "AREF" thru_hole oval (at 39.06 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-PadAREF)") (pinfunction "AREF") (pintype "power_in+no_connect") (tstamp 797525d5-379a-4e34-a5a9-e0af7409bc11))
    (pad "GND" thru_hole oval (at 11.12 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-PadGND)") (pinfunction "GND") (pintype "power_in") (tstamp 1f0c2da3-b236-4f08-b622-0e07ccb551c5))
    (pad "GND" thru_hole oval (at 16.2 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-PadGND)") (pinfunction "GND") (pintype "power_in") (tstamp 769f21aa-cb33-4d2a-a3bf-2d9bc07de169))
    (pad "MI" thru_hole oval (at 6.04 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-PadMI)") (pinfunction "MISO") (pintype "bidirectional+no_connect") (tstamp d05d499d-ce2c-460a-b4d7-df3cd1e8b539))
    (pad "MO" thru_hole rect (at 3.5 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-PadMO)") (pinfunction "MOSI") (pintype "bidirectional+no_connect") (tstamp dd77798f-dcaa-491b-adf7-bf9b46051fca))
    (pad "NC" thru_hole oval (at 21.28 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-PadNC)") (pintype "no_connect") (tstamp 7caa9d2f-447f-4877-9fc2-1d1e4ffb2f34))
    (pad "NC" thru_hole oval (at 18.74 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-PadNC)") (pintype "no_connect") (tstamp c0983c7a-cf6d-4fe3-ab4e-da3e141bc74e))
    (pad "RST" thru_hole oval (at 13.66 1.254 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-PadRST)") (pinfunction "RESET") (pintype "bidirectional+no_connect") (tstamp 536edd23-e6d9-4398-bbdc-8bdcb2cd0324))
    (pad "RST" thru_hole oval (at 13.66 16.51 90) (size 1.7 3) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-PadRST)") (pinfunction "RESET") (pintype "bidirectional+no_connect") (tstamp 640e3ddd-9602-4b23-8b23-cf29b39e3478))
    (pad "RX" thru_hole oval (at 11.12 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U1-PadRX)") (pinfunction "0/RX") (pintype "bidirectional+no_connect") (tstamp 29dd39ec-0593-4bec-a585-50a0654847ae))
    (pad "SCK" thru_hole oval (at 3.5 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U1-PadSCK)") (pinfunction "SCK") (pintype "bidirectional+no_connect") (tstamp 8c8447cb-0a37-43b7-bf9d-7fd77f29108d))
    (pad "SS" thru_hole oval (at 6.04 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U1-PadSS)") (pinfunction "RX_LED/SS") (pintype "bidirectional+no_connect") (tstamp 3d92292f-9c66-472a-a3e1-b58890490623))
    (pad "TX" thru_hole oval (at 8.58 1.254 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U1-PadTX)") (pinfunction "1/TX") (pintype "bidirectional+no_connect") (tstamp 87220fbf-2f72-4f01-a8fe-267b9a16b562))
    (pad "VI" thru_hole oval (at 8.58 16.51 90) (size 2 3) (drill 1) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U1-PadVI)") (pinfunction "VIN") (pintype "power_in+no_connect") (tstamp c0632509-1161-4361-802b-6525b786cf8f))
    (model "M:/arduino-micro-3.snapshot.9/arduino_micro.STEP" hide
      (offset (xyz -0.5 18 2.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "M:/ARDUINO MICRO.STEP"
      (offset (xyz 3.5 1.3 2.6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 6227A60F) (tstamp 7783caad-32e1-4cb9-a1e2-e38997af04a8)
    (at 182.375 76.475 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/8c077155-3d1b-4c61-8ad6-aa7da49ff67a")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.33 90) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 032b025e-949e-4927-ac7f-cb13999d76b1)
    )
    (fp_text value "Conn_01x06" (at -2.525 -9.875 180) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e3905afb-f595-419b-bf7d-21c586978025)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 24e0d778-e59a-460f-afdb-3c30ce14b0a2)
    )
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp 0300ad45-6dca-4f5d-a764-9d9f4357f09a))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp 4eba73c1-22c1-4a07-b602-681475a08395))
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 5497b345-8fa4-4bf0-96f7-f417951e39b4))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp bbf27c9c-d5fc-41b4-830f-bfc488bff3fc))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp e7340c0c-f1b1-443c-aed2-c3c18033b2bb))
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp eb3e1c72-8175-4c09-8fda-413b03a4d358))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 6f75e63c-1453-459c-8f70-5a028d2a0923))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 7bd182cc-8f9f-493c-9c52-eec5e4b7c1f5))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp ea0b41d2-99cc-47db-852c-750294fed629))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp fbbc41da-2fcc-48a6-9a07-0abc4a17b166))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 38668abb-13b0-4d64-9754-1cdf0a1f230f))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp 48311f5e-0e8c-42c4-b39d-9ff005975267))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 6876bb00-939a-4e42-abfb-a049fe5d0231))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp ebce33c4-45be-4c9f-9a90-59cc8502d061))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp f3caba9a-f88e-44a3-bd8f-904f683312b6))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 30edbf08-b311-44bc-b637-a1991c3dc589))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp e319d4dc-0cb6-4e65-bc65-7f9c1bb431d5))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp cc39063c-5598-47a9-b378-b2eb02abffd8))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 418c847e-f0da-4757-a0e8-bae6a0dfb47b))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 8b0bf5cd-e319-4f51-9399-a740349ec446))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp 613795a2-5dac-4dc9-b0f7-371c54ba440e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (gr_line (start 108 73.5) (end 108 80) (layer "Edge.Cuts") (width 0.1) (tstamp 0cc20d10-da49-4751-8aec-79279d1ad7ad))
  (gr_line (start 185 73.5) (end 185 80) (layer "Edge.Cuts") (width 0.1) (tstamp 2fffe151-1e8a-4e47-b673-6a8ca3555650))
  (gr_line (start 135 122) (end 158 122) (layer "Edge.Cuts") (width 0.1) (tstamp 79182a58-76fc-4e26-aa73-bab841dd1efd))
  (gr_line (start 108 80) (end 135 122) (layer "Edge.Cuts") (width 0.1) (tstamp 7e4d0370-d586-4bf4-ab42-5afd41b4978a))
  (gr_line (start 185 80) (end 158 122) (layer "Edge.Cuts") (width 0.1) (tstamp 9be1299c-3059-4a81-88a6-86a98bd41ce1))
  (gr_line (start 108 73.5) (end 185 73.5) (layer "Edge.Cuts") (width 0.1) (tstamp cc850dc5-b03e-4031-9fe6-82f8450f7cf8))

  (segment (start 113.04 78.04) (end 118 83) (width 0.5) (layer "F.Cu") (net 1) (tstamp 25151b61-692f-41ce-b787-3a444fc3fa01))
  (segment (start 132.5 101.4255) (end 133.75 102.6755) (width 0.5) (layer "F.Cu") (net 1) (tstamp 405a55c9-1fc1-4661-8533-6d7b38368b5e))
  (segment (start 118 83) (end 131.5 83) (width 0.5) (layer "F.Cu") (net 1) (tstamp 48bcdbf2-258b-4e30-bc94-14778eea72c7))
  (segment (start 132.5 84) (end 132.5 101.4255) (width 0.5) (layer "F.Cu") (net 1) (tstamp 72b9f027-5b18-4c95-8c72-b32efc315d70))
  (segment (start 133.75 102.6755) (end 138.8415 102.6755) (width 0.5) (layer "F.Cu") (net 1) (tstamp 78a1ef7f-c2d5-4c6b-9982-4e130942eea1))
  (segment (start 131.5 83) (end 132.5 84) (width 0.5) (layer "F.Cu") (net 1) (tstamp ba7173ad-9a10-4235-b92a-13a57975dc32))
  (segment (start 113.04 76.5) (end 113.04 78.04) (width 0.5) (layer "B.Cu") (net 1) (tstamp dea877d3-8331-4b13-8baa-7d5e65a7669b))
  (segment (start 115.58 78.08) (end 119.5 82) (width 0.5) (layer "F.Cu") (net 2) (tstamp 06bfdbdf-3e53-42a3-abc9-fd9ec56e91ec))
  (segment (start 132 82) (end 133.5 83.5) (width 0.5) (layer "F.Cu") (net 2) (tstamp 7e517a6d-aeab-459a-b195-aad471920d40))
  (segment (start 133.5 83.5) (end 133.5 98.6355) (width 0.5) (layer "F.Cu") (net 2) (tstamp 87c68946-be6c-4b47-bb86-336211c62204))
  (segment (start 133.5 98.6355) (end 135 100.1355) (width 0.5) (layer "F.Cu") (net 2) (tstamp b9272d3e-f4bd-4317-80a0-74d47b78e9d0))
  (segment (start 135 100.1355) (end 138.8415 100.1355) (width 0.5) (layer "F.Cu") (net 2) (tstamp bde59edb-ae26-40ab-9f84-4abf28de2a39))
  (segment (start 119.5 82) (end 132 82) (width 0.5) (layer "F.Cu") (net 2) (tstamp db8aafef-e19a-420b-88b7-043a52d677fa))
  (segment (start 115.58 76.5) (end 115.58 78.08) (width 0.5) (layer "B.Cu") (net 2) (tstamp cd1ec840-a9ae-4348-8e74-0ea5ea214714))
  (segment (start 121 81) (end 132.5 81) (width 0.5) (layer "F.Cu") (net 4) (tstamp 1d17904d-638f-48f3-894f-0144911f4a7c))
  (segment (start 132.5 81) (end 134.5 83) (width 0.5) (layer "F.Cu") (net 4) (tstamp 4f93e57a-6ce8-405a-a3be-33c04d949cd8))
  (segment (start 134.5 96.3455) (end 135.75 97.5955) (width 0.5) (layer "F.Cu") (net 4) (tstamp 5000856e-be88-4ba5-a96b-fce607847f2e))
  (segment (start 118.12 78.12) (end 121 81) (width 0.5) (layer "F.Cu") (net 4) (tstamp 7a853ac3-05dc-426c-b339-3fd8fe77ab83))
  (segment (start 135.75 97.5955) (end 138.8415 97.5955) (width 0.5) (layer "F.Cu") (net 4) (tstamp 9b2d1805-884a-452f-9983-194da6f596e2))
  (segment (start 134.5 83) (end 134.5 96.3455) (width 0.5) (layer "F.Cu") (net 4) (tstamp a857533f-9202-4f5b-bf5f-10237709afa0))
  (segment (start 118.12 76.5) (end 118.12 78.12) (width 0.5) (layer "B.Cu") (net 4) (tstamp 9f7d6bfc-d101-4f0a-a424-a1bfc7491cb4))
  (segment (start 120.66 78.16) (end 122.5 80) (width 0.5) (layer "F.Cu") (net 5) (tstamp 0fb612b6-d118-463f-8273-72d16ac7c8f3))
  (segment (start 122.5 80) (end 133 80) (width 0.5) (layer "F.Cu") (net 5) (tstamp 543ccabc-4148-495e-bbf3-b3f2d2fb3d9e))
  (segment (start 136.5555 95.0555) (end 138.8415 95.0555) (width 0.5) (layer "F.Cu") (net 5) (tstamp 700c69dc-6ed3-40ed-ad9c-7efb2c64ff49))
  (segment (start 133 80) (end 135.5 82.5) (width 0.5) (layer "F.Cu") (net 5) (tstamp 9d79fbcb-66f8-4fdd-981b-13682af2e9c2))
  (segment (start 135.5 82.5) (end 135.5 94) (width 0.5) (layer "F.Cu") (net 5) (tstamp c2c90718-4d9f-4ef5-81a7-15980c454fb8))
  (segment (start 135.5 94) (end 136.5555 95.0555) (width 0.5) (layer "F.Cu") (net 5) (tstamp f891d608-0631-4563-b6da-cbd3d620af2b))
  (segment (start 120.66 76.5) (end 120.66 78.16) (width 0.5) (layer "B.Cu") (net 5) (tstamp f899bfea-cd85-4f68-bcb7-163efe1686d6))
  (segment (start 154.0975 105.2155) (end 152.2155 105.2155) (width 0.5) (layer "F.Cu") (net 6) (tstamp 0f1d963c-6d4c-4135-aa25-249e05c4978c))
  (segment (start 151.5 104.5) (end 152.2155 105.2155) (width 0.5) (layer "F.Cu") (net 6) (tstamp 352d0d28-f0d2-4708-bba2-8de37f80ba70))
  (segment (start 153 75.5) (end 168.7 75.5) (width 0.5) (layer "F.Cu") (net 6) (tstamp 42978a20-0456-4cd6-8083-d85e104e9a1c))
  (segment (start 151.5 77) (end 151.5 104.5) (width 0.5) (layer "F.Cu") (net 6) (tstamp dd6d1468-3a3b-4984-8dbf-639687a184e3))
  (segment (start 153 75.5) (end 151.5 77) (width 0.5) (layer "F.Cu") (net 6) (tstamp e71169c0-a25b-4c6e-a8d2-4453f8ff30b2))
  (segment (start 168.7 75.5) (end 169.675 76.475) (width 0.5) (layer "B.Cu") (net 6) (tstamp 92ceac64-70ab-4b89-8ada-2550eb9b25fe))
  (segment (start 124.5 79) (end 133.5 79) (width 0.5) (layer "F.Cu") (net 7) (tstamp 30a5898d-4bac-46ac-b409-1a5087097191))
  (segment (start 136.5 92) (end 137.0155 92.5155) (width 0.5) (layer "F.Cu") (net 7) (tstamp 677b8ad7-c9ad-4d6d-ab0e-0b522c3f53fa))
  (segment (start 133.5 79) (end 136.5 82) (width 0.5) (layer "F.Cu") (net 7) (tstamp a159a55b-d7c9-48c5-b99b-321f67c98e97))
  (segment (start 136.5 82) (end 136.5 92) (width 0.5) (layer "F.Cu") (net 7) (tstamp affb5435-28c4-4f06-9b4a-99f62a3ddd61))
  (segment (start 123.2 77.7) (end 124.5 79) (width 0.5) (layer "F.Cu") (net 7) (tstamp e6e34111-36ab-4857-956c-628227e5add3))
  (segment (start 137.5155 92.5155) (end 138.8415 92.5155) (width 0.5) (layer "B.Cu") (net 7) (tstamp 197e2dd9-da7b-4445-8419-f4df75d6cb82))
  (segment (start 123.2 76.5) (end 123.2 77.7) (width 0.5) (layer "B.Cu") (net 7) (tstamp 369da08e-6ca7-4f68-b9d3-c0a8e8b95ae7))
  (segment (start 156.5 80) (end 156.5 83.75) (width 0.5) (layer "F.Cu") (net 15) (tstamp 1ad69de7-3069-4816-80ad-6cd0aaa9520d))
  (segment (start 172.215 77.785) (end 171.5 78.5) (width 0.5) (layer "F.Cu") (net 15) (tstamp 2b2e9c72-e284-4c5f-8c21-a8e12a7afaa6))
  (segment (start 155.3955 84.8955) (end 156.5 83.791) (width 0.5) (layer "F.Cu") (net 15) (tstamp 67d6f90c-783e-4f0c-af06-9383169c670c))
  (segment (start 158 78.5) (end 156.5 80) (width 0.5) (layer "F.Cu") (net 15) (tstamp a4aca7af-7e01-4d33-9da4-6a10445f9924))
  (segment (start 171.5 78.5) (end 158 78.5) (width 0.5) (layer "F.Cu") (net 15) (tstamp c31e94f6-ea59-4f8b-836c-962b906b3567))
  (segment (start 172.215 76.475) (end 172.215 77.785) (width 0.5) (layer "B.Cu") (net 15) (tstamp 53f79363-0a49-485e-a7c0-9bbb001293f4))
  (segment (start 153.993 85) (end 154.0975 84.8955) (width 0.5) (layer "B.Cu") (net 15) (tstamp 5f7ef96b-c911-4558-8877-98384e06af8f))
  (segment (start 155.3955 84.8955) (end 154.0975 84.8955) (width 0.5) (layer "B.Cu") (net 15) (tstamp fe7d0f6f-61b6-4613-b6b4-2ca494de34f9))
  (segment (start 157.5 86.5) (end 156.5645 87.4355) (width 0.5) (layer "F.Cu") (net 16) (tstamp 2983eed3-ea9d-439e-9233-2d406b03c1b1))
  (segment (start 158.5 79.5) (end 157.5 80.5) (width 0.5) (layer "F.Cu") (net 16) (tstamp 34f21fa6-97cb-46f0-9355-732855088623))
  (segment (start 174.755 76.475) (end 174.755 78.245) (width 0.5) (layer "F.Cu") (net 16) (tstamp 3bef48a0-80c5-4045-ae33-618d338dc112))
  (segment (start 174.755 78.245) (end 173.5 79.5) (width 0.5) (layer "F.Cu") (net 16) (tstamp 7abd4a40-312a-44bc-837d-0d0f6e321200))
  (segment (start 157.5 80.5) (end 157.5 86.5) (width 0.5) (layer "F.Cu") (net 16) (tstamp b2df3f6c-4c89-4cdc-b52d-575e83751794))
  (segment (start 156.5645 87.4355) (end 154.0975 87.4355) (width 0.5) (layer "F.Cu") (net 16) (tstamp bd6b5f42-d199-4e65-8646-3802e7b18d68))
  (segment (start 173.5 79.5) (end 158.5 79.5) (width 0.5) (layer "F.Cu") (net 16) (tstamp c4b17d67-f3ce-4b8a-a94d-16663a3e542c))
  (segment (start 156.5245 89.9755) (end 154.0975 89.9755) (width 0.5) (layer "F.Cu") (net 17) (tstamp 13b2d13f-6e57-4a66-89cb-393eb23542ce))
  (segment (start 177.295 78.705) (end 175 81) (width 0.5) (layer "F.Cu") (net 17) (tstamp 3a790a8a-e886-4c69-acac-163cf8319b7f))
  (segment (start 177.295 76.475) (end 177.295 78.705) (width 0.5) (layer "F.Cu") (net 17) (tstamp 4fa27394-0095-4348-aec9-6738834cb164))
  (segment (start 159 81.5) (end 159 87.5) (width 0.5) (layer "F.Cu") (net 17) (tstamp 73b1f676-64a1-4437-9380-52c422752ac5))
  (segment (start 159 87.5) (end 156.5245 89.9755) (width 0.5) (layer "F.Cu") (net 17) (tstamp 98fbf647-1162-43ea-b928-4f63a66416b1))
  (segment (start 175 81) (end 159.5 81) (width 0.5) (layer "F.Cu") (net 17) (tstamp 9b045781-f35d-4c58-a40d-2987f7c8f201))
  (segment (start 159.5 81) (end 159 81.5) (width 0.5) (layer "F.Cu") (net 17) (tstamp b696f93a-2d3f-4f8f-bf9a-d8a5df9b1cca))
  (segment (start 160.5 89) (end 156.9845 92.5155) (width 0.5) (layer "F.Cu") (net 18) (tstamp 2af49a64-5275-4a14-9e41-662b70ae83e7))
  (segment (start 176.5 82.5) (end 161.5 82.5) (width 0.5) (layer "F.Cu") (net 18) (tstamp 2ee56b50-7a2e-4579-847e-d50ffb24bfa7))
  (segment (start 160.5 83.5) (end 160.5 89) (width 0.5) (layer "F.Cu") (net 18) (tstamp 38d40f93-6d00-4e2c-94b7-94c7d6758dca))
  (segment (start 179.835 79.165) (end 176.5 82.5) (width 0.5) (layer "F.Cu") (net 18) (tstamp 6e8cdc15-1d87-40f0-8567-da30489099bd))
  (segment (start 156.9845 92.5155) (end 154.0975 92.5155) (width 0.5) (layer "F.Cu") (net 18) (tstamp 92aef758-0a96-47b7-a60e-163742d5f776))
  (segment (start 161.5 82.5) (end 160.5 83.5) (width 0.5) (layer "F.Cu") (net 18) (tstamp 9e1c18f8-5bd4-4de3-a601-efdd5380d879))
  (segment (start 179.835 76.475) (end 179.835 79.165) (width 0.5) (layer "F.Cu") (net 18) (tstamp fada9d7b-48cd-47e2-bdef-6fdf5e4e20a3))
  (segment (start 156.9445 95.0555) (end 154.0975 95.0555) (width 0.5) (layer "F.Cu") (net 19) (tstamp 24b5b5d8-bfba-4591-bb46-3d7cf0452c7d))
  (segment (start 178 84) (end 163 84) (width 0.5) (layer "F.Cu") (net 19) (tstamp 36ab21de-a592-4b81-9469-549bd1466958))
  (segment (start 182.375 76.475) (end 182.375 79.625) (width 0.5) (layer "F.Cu") (net 19) (tstamp 3752bd70-1b60-4811-a0ab-8f738708853d))
  (segment (start 162 90) (end 156.9445 95.0555) (width 0.5) (layer "F.Cu") (net 19) (tstamp 5e0db56b-9a17-478a-a918-a065c8bf2944))
  (segment (start 162 85) (end 162 90) (width 0.5) (layer "F.Cu") (net 19) (tstamp 6c8c5047-8d7d-4efe-80aa-e9e65c4097f8))
  (segment (start 182.375 79.625) (end 178 84) (width 0.5) (layer "F.Cu") (net 19) (tstamp 95443a11-53f4-4425-8c94-10254655208f))
  (segment (start 163 84) (end 162 85) (width 0.5) (layer "F.Cu") (net 19) (tstamp ca685e90-2e2a-4112-9b72-319df3473d4d))
  (segment (start 182.375 76.475) (end 182.375 75.875) (width 0.5) (layer "B.Cu") (net 19) (tstamp 1306c8bf-ff29-43d8-9cba-26f27e067ac9))
  (segment (start 131.5 103.7155) (end 133 105.2155) (width 0.5) (layer "F.Cu") (net 22) (tstamp 10287a93-f2ea-4f9e-9400-e99b64e4e5d1))
  (segment (start 143.2155 105.2155) (end 148.2955 110.2955) (width 0.5) (layer "F.Cu") (net 22) (tstamp 28eb196c-bac9-4b0f-ad9f-1330c6f95cf7))
  (segment (start 133 105.2155) (end 138.8415 105.2155) (width 0.5) (layer "F.Cu") (net 22) (tstamp 38308367-4562-4a6a-bd15-9e81dd42d931))
  (segment (start 110.5 78) (end 116.5 84) (width 0.5) (layer "F.Cu") (net 22) (tstamp 67b9688c-3b8f-4eb9-810c-07fbc4793323))
  (segment (start 116.5 84) (end 131 84) (width 0.5) (layer "F.Cu") (net 22) (tstamp 8458b7b0-3f5c-4803-ac1b-eac2ca1fefe9))
  (segment (start 148.2955 110.2955) (end 154.0975 110.2955) (width 0.5) (layer "F.Cu") (net 22) (tstamp 851b0579-5f25-4ef5-8dec-a9dab7b92d0c))
  (segment (start 131 84) (end 131.5 84.5) (width 0.5) (layer "F.Cu") (net 22) (tstamp 98476643-1dc3-4cb2-875f-ffa29d752e72))
  (segment (start 138.8415 105.2155) (end 143.2155 105.2155) (width 0.5) (layer "F.Cu") (net 22) (tstamp bbbc389f-fc56-4114-8dca-829a896f23b3))
  (segment (start 131.5 84.5) (end 131.5 103.7155) (width 0.5) (layer "F.Cu") (net 22) (tstamp de6ff3c0-1771-444c-8aae-986eb6a26dec))
  (segment (start 110.5 76.5) (end 110.5 78) (width 0.5) (layer "B.Cu") (net 22) (tstamp f02620e3-bfa8-4381-b81b-d3dde8ba342c))
  (segment (start 154.0975 100.1355) (end 154.0975 102.6755) (width 2) (layer "F.Cu") (net 25) (tstamp 9db20b29-eea9-4053-9877-76349882807a))
  (segment (start 138.8415 107.7555) (end 142.7555 107.7555) (width 0.5) (layer "F.Cu") (net 26) (tstamp 065e1ae2-ca87-4007-8bf4-c79c0db5ccc2))
  (segment (start 147 120) (end 155.5 120) (width 0.5) (layer "F.Cu") (net 26) (tstamp 19a547a3-3c1b-4cb4-b542-87c409928a1e))
  (segment (start 145 110) (end 145 118) (width 0.5) (layer "F.Cu") (net 26) (tstamp 29ba63ff-0016-489e-892b-218e7b0455f6))
  (segment (start 145 118) (end 147 120) (width 0.5) (layer "F.Cu") (net 26) (tstamp 49bfd57e-86aa-4e62-8195-0f4ab8a6c89f))
  (segment (start 142.7555 107.7555) (end 145 110) (width 0.5) (layer "F.Cu") (net 26) (tstamp 5e90be12-c12d-4ef9-8792-3f9bcfb29f9e))
  (segment (start 157 109.5) (end 155.2555 107.7555) (width 0.5) (layer "F.Cu") (net 26) (tstamp 98cd4b13-6177-4821-9181-9529256987cb))
  (segment (start 155.5 120) (end 157 118.5) (width 0.5) (layer "F.Cu") (net 26) (tstamp c194e6df-c2ed-45fe-957c-94a4e155c8e3))
  (segment (start 157 118.5) (end 157 109.5) (width 0.5) (layer "F.Cu") (net 26) (tstamp cd19d8af-ddf4-49bd-8bbd-580223e04c2f))
  (segment (start 155.2555 107.7555) (end 154.0975 107.7555) (width 0.5) (layer "B.Cu") (net 26) (tstamp ee9bf8ce-1090-4589-b782-9a2c664c24ae))

)
