(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001000_7fffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers")
    )
  )

  (net 0 "")
  (net 1 "Net-(J2-Pad5)")
  (net 2 "Net-(J2-Pad4)")
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "unconnected-(U1-Pad1)")
  (net 7 "unconnected-(U1-Pad2)")
  (net 8 "unconnected-(U1-Pad3)")
  (net 9 "unconnected-(U1-Pad5)")
  (net 10 "unconnected-(U1-Pad6)")
  (net 11 "unconnected-(U1-Pad7)")
  (net 12 "unconnected-(U1-Pad18)")
  (net 13 "unconnected-(U1-Pad19)")
  (net 14 "unconnected-(U1-Pad20)")
  (net 15 "unconnected-(U1-Pad23)")
  (net 16 "unconnected-(U1-Pad24)")
  (net 17 "Net-(U1-Pad14)")
  (net 18 "unconnected-(U1-Pad22)")
  (net 19 "Net-(U1-Pad4)")
  (net 20 "Net-(U1-Pad21)")
  (net 21 "Net-(U1-Pad17)")
  (net 22 "Net-(U1-Pad16)")
  (net 23 "Net-(U1-Pad15)")
  (net 24 "Net-(U1-Pad13)")

  (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 623B7E9E) (tstamp 386a0090-0a46-4bfb-96d1-b3d435c60ba8)
    (at 15.2 -29 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/8c077155-3d1b-4c61-8ad6-aa7da49ff67a")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.33 270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5ab39f29-a99d-4137-813c-0240aaa35e79)
    )
    (fp_text value "Conn_01x06" (at 0 -15.03 270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e843b2f9-63bf-4162-9acd-99c55f41dac5)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 82e9af86-fd44-49c7-8996-479996b9b858)
    )
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp 28d92791-e03b-49b7-ab76-0b79e48b37f2))
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 2fe8fb82-a875-43d9-b72f-82742b7cdb00))
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 6c738b90-c565-4419-b3f8-c71fa068a959))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp a5860b45-4fc2-46a1-acd5-e3fbb8cba155))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp c8c88636-920e-4be2-a4e2-fc3f7ddd659c))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp e9ea7cf3-811f-4d45-affd-39be4058ac53))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 4a8a7ae8-e1f4-43bc-bf27-d27128fb055b))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 5dfe42c6-01b7-4abd-b9a5-6c91c2956ce9))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp d0a1fb4e-1977-4087-a971-99b683cf87ba))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp d4de041b-b58a-4daa-beee-c967a97f2743))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp 20afe9c7-7e63-485a-bab2-9fad3cd73f01))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 35cdb7da-6207-458e-b9a0-57079b9acb1f))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 41d14a77-a1a1-4f82-be40-67934bda1603))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp ba8befbb-68c6-431f-9d30-3f3bf9a6b7e3))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp c9ad0256-e795-473a-9d31-5442242d3188))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad21)") (pinfunction "Pin_1") (pintype "passive") (tstamp 18c97c17-4686-4762-ac2f-547b5b999ca9))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad17)") (pinfunction "Pin_2") (pintype "passive") (tstamp 519527ee-f2dc-482d-94bb-75721ed8aafb))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad16)") (pinfunction "Pin_3") (pintype "passive") (tstamp c7878c4f-2f8a-4bbb-adbc-833e5b6f7423))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad15)") (pinfunction "Pin_4") (pintype "passive") (tstamp 5ca1b4f0-e4cd-4f1a-9bfa-ba57d20cfd00))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad14)") (pinfunction "Pin_5") (pintype "passive") (tstamp 8f6e74de-71c3-4969-bfa3-21ee2db29d12))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad13)") (pinfunction "Pin_6") (pintype "passive") (tstamp 56486356-64f4-4148-b335-6b45c342341d))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 623B7ECA) (tstamp 7783caad-32e1-4cb9-a1e2-e38997af04a8)
    (at 74.375 -29 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/abc425ae-34db-440c-baf2-199506429483")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.33 270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cc4f0b33-ccfd-419b-9659-a88488fda9d5)
    )
    (fp_text value "Conn_01x06" (at 0 -15.03 270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c93092f3-ad93-4616-a7d6-461e3ba02b31)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4770ef60-21bb-4d72-93b1-855cef6e8fb9)
    )
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 209b39ed-1521-46f3-985b-6f682af8a636))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp 23b01e04-7511-4c52-80ed-871675300ee9))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp 42f5b5b4-dd5c-4778-98da-3fe6b6b36b6c))
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp a001f9b3-d55c-45e5-82b3-54c3c57f50f4))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp a12176d4-cccd-4936-bd41-2b7cdce20b70))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp d5ed5e46-d54a-447d-9f4b-f0768c1fbc9a))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 0fb612b6-d118-463f-8273-72d16ac7c8f3))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 3825ef5a-9c20-4da1-b237-0d7cce88677d))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 524dfc74-a6ca-4f47-b1c4-8c830a3897c9))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp cef8d6fd-fad1-4b1e-bfe8-44b8b9fd4ec5))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp 207c4811-314a-47bb-ae18-2f9379831b81))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 241d45c3-e292-4286-88e2-648d09936352))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp 543ccabc-4148-495e-bbf3-b3f2d2fb3d9e))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 789fde59-6346-41c4-8bdd-f9aa5fd7f3db))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 89e85ee3-bf08-4d94-97ac-77b0e3f043c9))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 2ff20828-bd59-4b9f-96ee-57d97ba845ab))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 756c320d-1757-4c24-8d25-eea4479fc01c))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp 35301f71-3327-4814-addd-6803f155857b))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp dddee525-5a91-4e7c-9753-319ed47ddcc0))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 008d03ef-d971-462c-bfb3-7aa302eab0fd))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad4)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7ac680eb-02c3-488d-9052-a4bda05e99dd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Creadas:ProMicro" (layer "B.Cu")
    (tedit 623B8046) (tstamp c1b78138-c11c-4fb6-bc53-1e102c698b86)
    (at 38.5 -15.73 -90)
    (descr "Pro Micro footprint")
    (tags "promicro ProMicro")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/c71f56c1-5b7c-4373-9716-fffac482104c")
    (attr through_hole)
    (fp_text reference "U1" (at 0 10.16 90) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2135eddd-f41f-4ab2-a263-8dadf6425926)
    )
    (fp_text value "ProMicro" (at 0 -10.16 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 642c3167-61ff-412b-b7c2-23be8f7d6d81)
    )
    (fp_line (start -15.24 -8.89) (end 15.24 -8.89) (layer "B.SilkS") (width 0.15) (tstamp 02b95530-09eb-4a8e-a488-67c549fc95da))
    (fp_line (start -15.24 8.89) (end 15.24 8.89) (layer "B.SilkS") (width 0.15) (tstamp 1cd8e2a0-99d1-450c-aa49-c54d9399ba6b))
    (fp_line (start -15.24 -8.89) (end -15.24 -3.81) (layer "B.SilkS") (width 0.15) (tstamp 3e368736-42ee-49e8-b8e6-92f23d085d37))
    (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer "B.SilkS") (width 0.15) (tstamp aed1af86-2fd4-47a3-a678-1eaf5b9cda50))
    (fp_line (start -17.78 -3.81) (end -17.78 3.81) (layer "B.SilkS") (width 0.15) (tstamp b82d984a-2a78-4dbf-9516-5c16648505e3))
    (fp_line (start -15.24 -3.81) (end -17.78 -3.81) (layer "B.SilkS") (width 0.15) (tstamp deca1926-78fc-4dc2-8b2d-b454284b8ba9))
    (fp_line (start -15.24 3.81) (end -15.24 8.89) (layer "B.SilkS") (width 0.15) (tstamp e190aa7b-5147-4d85-8d47-de2af4e5add9))
    (fp_line (start -17.78 3.81) (end -15.24 3.81) (layer "B.SilkS") (width 0.15) (tstamp f195d16d-ee5a-46c9-bfed-922f99074f3e))
    (pad "1" thru_hole rect (at -13.97 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 6 "unconnected-(U1-Pad1)") (pinfunction "TX") (pintype "bidirectional+no_connect") (tstamp 20ded32e-6cec-4642-9bbf-bec8a4313054))
    (pad "2" thru_hole oval (at -11.43 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 7 "unconnected-(U1-Pad2)") (pinfunction "RX") (pintype "bidirectional+no_connect") (tstamp e444c522-353b-4c32-a29c-27f7d80eb8d7))
    (pad "3" thru_hole oval (at -8.89 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 8 "unconnected-(U1-Pad3)") (pinfunction "GND") (pintype "power_in+no_connect") (tstamp db3b5812-159f-4218-aac7-75d053a4d199))
    (pad "4" thru_hole oval (at -6.35 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 19 "Net-(U1-Pad4)") (pinfunction "GND") (pintype "power_in") (tstamp 830d8dfa-69fa-4cf9-8d51-65cceb582110))
    (pad "5" thru_hole oval (at -3.81 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 9 "unconnected-(U1-Pad5)") (pinfunction "SDA") (pintype "bidirectional+no_connect") (tstamp 89061b42-bdae-4630-82ba-272670b4f27d))
    (pad "6" thru_hole oval (at -1.27 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 10 "unconnected-(U1-Pad6)") (pinfunction "SCL") (pintype "bidirectional+no_connect") (tstamp 14816cdb-f803-40c8-89cf-68b16fa15c10))
    (pad "7" thru_hole oval (at 1.27 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 11 "unconnected-(U1-Pad7)") (pinfunction "D4") (pintype "bidirectional+no_connect") (tstamp 48e5b7a6-0e4d-4865-a203-7b9471d025f7))
    (pad "8" thru_hole oval (at 3.81 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 1 "Net-(J2-Pad5)") (pinfunction "C6") (pintype "bidirectional") (tstamp ad40c983-f57f-4b8e-a3bf-b2b9aacd6fea))
    (pad "9" thru_hole oval (at 6.35 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 2 "Net-(J2-Pad4)") (pinfunction "D7") (pintype "bidirectional") (tstamp a66818c8-2ced-42b9-b3bf-b5a68a2926fb))
    (pad "10" thru_hole oval (at 8.89 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 3 "Net-(J2-Pad3)") (pinfunction "E6") (pintype "bidirectional") (tstamp 0afa9efe-7d2f-4a19-99dd-8dcd3edb1ab5))
    (pad "11" thru_hole oval (at 11.43 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 4 "Net-(J2-Pad2)") (pinfunction "B4") (pintype "bidirectional") (tstamp b400ebaf-6b57-44f1-9567-307212111260))
    (pad "12" thru_hole oval (at 13.97 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 5 "Net-(J2-Pad1)") (pinfunction "B5") (pintype "bidirectional") (tstamp 51fb00d7-24f9-4376-8d7b-c05ca25bcc28))
    (pad "13" thru_hole oval (at 13.97 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 24 "Net-(U1-Pad13)") (pinfunction "B6") (pintype "bidirectional") (tstamp 9bb640fc-fb87-47c3-ac83-b57dadd051cb))
    (pad "14" thru_hole oval (at 11.43 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 17 "Net-(U1-Pad14)") (pinfunction "B2") (pintype "bidirectional") (tstamp cbedae76-c5ff-4803-b4b9-c87aabd0a33f))
    (pad "15" thru_hole oval (at 8.89 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 23 "Net-(U1-Pad15)") (pinfunction "B3") (pintype "bidirectional") (tstamp 218f9185-7f56-42e5-8e76-84479290cb98))
    (pad "16" thru_hole oval (at 6.35 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 22 "Net-(U1-Pad16)") (pinfunction "B1") (pintype "bidirectional") (tstamp faa7310e-7d63-48e4-99eb-3069816753f0))
    (pad "17" thru_hole oval (at 3.81 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 21 "Net-(U1-Pad17)") (pinfunction "F7") (pintype "bidirectional") (tstamp d7328f0a-9d1b-4ed4-b09d-d92654faf8d8))
    (pad "18" thru_hole oval (at 1.27 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 12 "unconnected-(U1-Pad18)") (pinfunction "F6") (pintype "bidirectional+no_connect") (tstamp 0b3390cd-74f6-475b-9859-e721e89b07bd))
    (pad "19" thru_hole oval (at -1.27 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 13 "unconnected-(U1-Pad19)") (pinfunction "F5") (pintype "bidirectional+no_connect") (tstamp 82e16a6a-b2c8-4127-b702-a933d49a8632))
    (pad "20" thru_hole oval (at -3.81 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 14 "unconnected-(U1-Pad20)") (pinfunction "F4") (pintype "bidirectional+no_connect") (tstamp 283bb057-fadb-4943-99d0-ab38c6ed1303))
    (pad "21" thru_hole oval (at -6.35 7.62 270) (size 1.62 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 20 "Net-(U1-Pad21)") (pinfunction "VCC") (pintype "power_in") (tstamp 0d9713e7-b681-43f3-9e01-3339694f481d))
    (pad "22" thru_hole oval (at -8.89 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 18 "unconnected-(U1-Pad22)") (pinfunction "RST") (pintype "input+no_connect") (tstamp 331fc480-04a0-4bda-9dbb-20beb121452b))
    (pad "23" thru_hole oval (at -11.43 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 15 "unconnected-(U1-Pad23)") (pinfunction "GND") (pintype "power_in+no_connect") (tstamp 965c2489-f33d-47e8-9298-5a61e3c0971a))
    (pad "24" thru_hole oval (at -13.97 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 16 "unconnected-(U1-Pad24)") (pinfunction "RAW") (pintype "power_out+no_connect") (tstamp f66f9e8b-42f3-4267-b9bc-9a5e3781d428))
    (model "M:/ARDUINO PRO MICRO.STEP"
      (offset (xyz -13.95 -7.65 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (gr_line (start 0 0) (end 77 0) (layer "Edge.Cuts") (width 0.1) (tstamp 10c879d5-cd08-480e-8102-309b8ecea393))
  (gr_line (start 0 -31) (end 77 -31) (layer "Edge.Cuts") (width 0.15) (tstamp 7c55386f-d887-4962-bb89-7e762c57040b))
  (gr_line (start 0 -31) (end 0 0) (layer "Edge.Cuts") (width 0.1) (tstamp 96e75cf1-87d1-4b52-b945-bcd73be8c263))
  (gr_line (start 77 -31) (end 77 0) (layer "Edge.Cuts") (width 0.1) (tstamp fe651e19-573a-4fda-9b07-e9e295dc239b))
  (dimension (type aligned) (layer "Eco2.User") (tstamp cac811e8-03ed-4488-8c79-595617da12c8)
    (pts (xy 77 -31) (xy 0 -31))
    (height 3.5)
    (gr_text "77,0000 mm" (at 38.5 -35.65) (layer "Eco2.User") (tstamp cac811e8-03ed-4488-8c79-595617da12c8)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Eco2.User") (tstamp fa622127-2c8b-45a5-b225-aeabe299c2e5)
    (pts (xy 0 -31) (xy 0 0))
    (height 4)
    (gr_text "31,0000 mm" (at -5.15 -15.5 90) (layer "Eco2.User") (tstamp fa622127-2c8b-45a5-b225-aeabe299c2e5)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 61.42 -11.92) (end 46.12 -11.92) (width 1) (layer "F.Cu") (net 1) (tstamp 9e14b390-7235-46e6-96c7-f1d89b66ac03))
  (segment (start 64.215 -29) (end 64.215 -14.715) (width 1) (layer "F.Cu") (net 1) (tstamp e892b99b-bb53-407b-991a-48de4346a2f6))
  (segment (start 64.215 -14.715) (end 61.42 -11.92) (width 1) (layer "F.Cu") (net 1) (tstamp ee72f765-07f3-4e74-98fb-6dda5c1a40fb))
  (segment (start 66.755 -29) (end 66.755 -14.255) (width 1) (layer "F.Cu") (net 2) (tstamp 794b137c-7dcf-456f-ae2c-8a7797cf6255))
  (segment (start 61.88 -9.38) (end 46.12 -9.38) (width 1) (layer "F.Cu") (net 2) (tstamp 89d66050-8d51-40d3-a802-76f1be9afe92))
  (segment (start 66.755 -14.255) (end 61.88 -9.38) (width 1) (layer "F.Cu") (net 2) (tstamp d394c4a9-58eb-41d8-9bb8-30d31a96ca1c))
  (segment (start 69.295 -29) (end 69.295 -13.795) (width 1) (layer "F.Cu") (net 3) (tstamp 34f30412-602f-4141-9563-da13ebd80b15))
  (segment (start 69.295 -13.795) (end 62.34 -6.84) (width 1) (layer "F.Cu") (net 3) (tstamp 62c69777-a31e-4412-b338-d6838f91b3c2))
  (segment (start 62.34 -6.84) (end 46.12 -6.84) (width 1) (layer "F.Cu") (net 3) (tstamp 94a095b0-6f62-4e93-a799-588e263496bc))
  (segment (start 71.835 -13.335) (end 62.8 -4.3) (width 1) (layer "F.Cu") (net 4) (tstamp 675b03e2-3bd9-41a9-b07a-392c057f0196))
  (segment (start 71.835 -29) (end 71.835 -13.335) (width 1) (layer "F.Cu") (net 4) (tstamp b78fc0e1-5122-4f46-aa68-5238478f183f))
  (segment (start 62.8 -4.3) (end 46.12 -4.3) (width 1) (layer "F.Cu") (net 4) (tstamp ff48192e-40b0-4411-96e4-2f900d824e31))
  (segment (start 63.26 -1.76) (end 46.12 -1.76) (width 1) (layer "F.Cu") (net 5) (tstamp 39a48361-4dcc-4a8e-a09e-ef86f8cf177b))
  (segment (start 74.375 -12.875) (end 63.26 -1.76) (width 1) (layer "F.Cu") (net 5) (tstamp c38d87d2-40e2-4bc8-89ed-18d244da6f69))
  (segment (start 74.375 -29) (end 74.375 -12.875) (width 1) (layer "F.Cu") (net 5) (tstamp ee2d9f72-590f-429d-b65c-0b0cf86ed27c))
  (segment (start 5.04 -29) (end 5.04 -13.46) (width 1) (layer "F.Cu") (net 17) (tstamp 372b53a1-7603-44a3-980a-6d5305b84603))
  (segment (start 14.2 -4.3) (end 30.88 -4.3) (width 1) (layer "F.Cu") (net 17) (tstamp 7110880e-2ebb-461d-8917-9bd6d1ffddb6))
  (segment (start 5.04 -13.46) (end 14.2 -4.3) (width 1) (layer "F.Cu") (net 17) (tstamp ca19150f-fd40-4f2c-b308-2bc56457d600))
  (segment (start 61.675 -29) (end 61.675 -25.175) (width 1) (layer "F.Cu") (net 19) (tstamp a5d592ef-8b4a-454e-b240-b73bb1f112e5))
  (segment (start 58.58 -22.08) (end 46.12 -22.08) (width 1) (layer "F.Cu") (net 19) (tstamp b6195cbf-699e-40db-9354-a0d4d8daf71c))
  (segment (start 61.675 -25.175) (end 58.58 -22.08) (width 1) (layer "F.Cu") (net 19) (tstamp bd0ab73f-a93d-4cd6-81c7-2b78929b3a19))
  (segment (start 18.42 -22.08) (end 30.88 -22.08) (width 1) (layer "F.Cu") (net 20) (tstamp 06bf8433-3417-4ad2-bef4-1ea54d7858a8))
  (segment (start 15.2 -29) (end 15.2 -25.3) (width 1) (layer "F.Cu") (net 20) (tstamp 10dbed66-609a-4e15-85f4-97df95d48a55))
  (segment (start 15.2 -25.3) (end 18.42 -22.08) (width 1) (layer "F.Cu") (net 20) (tstamp d7aa4f28-3c7e-4681-84ee-2abd12835216))
  (segment (start 15.58 -11.92) (end 30.88 -11.92) (width 1) (layer "F.Cu") (net 21) (tstamp 17ea0eac-47ad-4665-b593-f2aa6d6648af))
  (segment (start 12.66 -29) (end 12.66 -14.84) (width 1) (layer "F.Cu") (net 21) (tstamp 3d1e9363-c8f2-48ea-a7a7-e788e690dd6b))
  (segment (start 12.66 -14.84) (end 15.58 -11.92) (width 1) (layer "F.Cu") (net 21) (tstamp 5722d0c0-bf1a-45e5-aeed-d22add7feb01))
  (segment (start 10.12 -14.38) (end 15.12 -9.38) (width 1) (layer "F.Cu") (net 22) (tstamp 2517d16b-4459-463e-9fa2-f4efc59d103a))
  (segment (start 10.12 -29) (end 10.12 -14.38) (width 1) (layer "F.Cu") (net 22) (tstamp 856f6596-24c7-47ce-af05-4c96cf721881))
  (segment (start 15.12 -9.38) (end 30.88 -9.38) (width 1) (layer "F.Cu") (net 22) (tstamp 8a641105-b9b5-4388-8b5f-d9d79a37df9e))
  (segment (start 7.58 -13.92) (end 14.66 -6.84) (width 1) (layer "F.Cu") (net 23) (tstamp 24394f05-03ed-4a33-8315-98f244d50619))
  (segment (start 14.66 -6.84) (end 30.88 -6.84) (width 1) (layer "F.Cu") (net 23) (tstamp 2e3bcf61-c850-4961-a682-3af35359032b))
  (segment (start 7.58 -29) (end 7.58 -13.92) (width 1) (layer "F.Cu") (net 23) (tstamp bc72b5b2-7af7-488d-b91b-58a1a8d3b9ab))
  (segment (start 2.5 -13) (end 13.74 -1.76) (width 1) (layer "F.Cu") (net 24) (tstamp 872893b7-d640-43de-92d7-86aff9e5a58a))
  (segment (start 13.74 -1.76) (end 30.88 -1.76) (width 1) (layer "F.Cu") (net 24) (tstamp ca68baa9-8d9e-4af0-b1cc-9d9fdf070771))
  (segment (start 2.5 -29) (end 2.5 -13) (width 1) (layer "F.Cu") (net 24) (tstamp caa91366-2091-49cb-8451-dd56e83f718f))

)
