(export (version "E")
  (design
    (source "I:\\Proyectos\\numPAD\\numPAD_MCU\\numPAD_MCU.kicad_sch")
    (date "23/03/2022 20:41:58")
    (tool "Eeschema (6.0.2)")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "numPAD_MCU.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "J1")
      (value "Conn_01x06")
      (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical")
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "8c077155-3d1b-4c61-8ad6-aa7da49ff67a"))
    (comp (ref "J2")
      (value "Conn_01x06")
      (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical")
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "abc425ae-34db-440c-baf2-199506429483"))
    (comp (ref "U1")
      (value "ProMicro")
      (footprint "Creadas:ProMicro")
      (libsource (lib "Creadas") (part "ProMicro") (description ""))
      (property (name "Sheetname") (value ""))
      (property (name "Sheetfile") (value "numPAD_MCU.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "c71f56c1-5b7c-4373-9716-fffac482104c")))
  (libparts
    (libpart (lib "Connector_Generic") (part "Conn_01x06")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x06")
        (field (name "Datasheet") "~"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))))
    (libpart (lib "Creadas") (part "ProMicro")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "ProMicro"))
      (pins
        (pin (num "1") (name "TX") (type "bidirectional"))
        (pin (num "2") (name "RX") (type "bidirectional"))
        (pin (num "3") (name "GND") (type "power_in"))
        (pin (num "4") (name "GND") (type "power_in"))
        (pin (num "5") (name "SDA") (type "bidirectional"))
        (pin (num "6") (name "SCL") (type "bidirectional"))
        (pin (num "7") (name "D4") (type "bidirectional"))
        (pin (num "8") (name "C6") (type "bidirectional"))
        (pin (num "9") (name "D7") (type "bidirectional"))
        (pin (num "10") (name "E6") (type "bidirectional"))
        (pin (num "11") (name "B4") (type "bidirectional"))
        (pin (num "12") (name "B5") (type "bidirectional"))
        (pin (num "13") (name "B6") (type "bidirectional"))
        (pin (num "14") (name "B2") (type "bidirectional"))
        (pin (num "15") (name "B3") (type "bidirectional"))
        (pin (num "16") (name "B1") (type "bidirectional"))
        (pin (num "17") (name "F7") (type "bidirectional"))
        (pin (num "18") (name "F6") (type "bidirectional"))
        (pin (num "19") (name "F5") (type "bidirectional"))
        (pin (num "20") (name "F4") (type "bidirectional"))
        (pin (num "21") (name "VCC") (type "power_in"))
        (pin (num "22") (name "RST") (type "input"))
        (pin (num "23") (name "GND") (type "power_in"))
        (pin (num "24") (name "RAW") (type "power_out")))))
  (libraries
    (library (logical "Connector_Generic")
      (uri "C:\\Program Files\\KiCad\\6.0\\share\\kicad\\symbols\\/Connector_Generic.kicad_sym"))
    (library (logical "Creadas")
      (uri "C:/Users/atanc/Documents/KiCad/6.0/symbols/Creadas.kicad_sym")))
  (nets
    (net (code "1") (name "Net-(J2-Pad1)")
      (node (ref "J2") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U1") (pin "12") (pinfunction "B5") (pintype "bidirectional")))
    (net (code "2") (name "Net-(J2-Pad2)")
      (node (ref "J2") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U1") (pin "11") (pinfunction "B4") (pintype "bidirectional")))
    (net (code "3") (name "Net-(J2-Pad3)")
      (node (ref "J2") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U1") (pin "10") (pinfunction "E6") (pintype "bidirectional")))
    (net (code "4") (name "Net-(J2-Pad4)")
      (node (ref "J2") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "9") (pinfunction "D7") (pintype "bidirectional")))
    (net (code "5") (name "Net-(J2-Pad5)")
      (node (ref "J2") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U1") (pin "8") (pinfunction "C6") (pintype "bidirectional")))
    (net (code "6") (name "Net-(U1-Pad4)")
      (node (ref "J2") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U1") (pin "4") (pinfunction "GND") (pintype "power_in")))
    (net (code "7") (name "Net-(U1-Pad13)")
      (node (ref "J1") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U1") (pin "13") (pinfunction "B6") (pintype "bidirectional")))
    (net (code "8") (name "Net-(U1-Pad14)")
      (node (ref "J1") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U1") (pin "14") (pinfunction "B2") (pintype "bidirectional")))
    (net (code "9") (name "Net-(U1-Pad15)")
      (node (ref "J1") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "15") (pinfunction "B3") (pintype "bidirectional")))
    (net (code "10") (name "Net-(U1-Pad16)")
      (node (ref "J1") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U1") (pin "16") (pinfunction "B1") (pintype "bidirectional")))
    (net (code "11") (name "Net-(U1-Pad17)")
      (node (ref "J1") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U1") (pin "17") (pinfunction "F7") (pintype "bidirectional")))
    (net (code "12") (name "Net-(U1-Pad21)")
      (node (ref "J1") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U1") (pin "21") (pinfunction "VCC") (pintype "power_in")))
    (net (code "13") (name "unconnected-(U1-Pad1)")
      (node (ref "U1") (pin "1") (pinfunction "TX") (pintype "bidirectional+no_connect")))
    (net (code "14") (name "unconnected-(U1-Pad2)")
      (node (ref "U1") (pin "2") (pinfunction "RX") (pintype "bidirectional+no_connect")))
    (net (code "15") (name "unconnected-(U1-Pad3)")
      (node (ref "U1") (pin "3") (pinfunction "GND") (pintype "power_in+no_connect")))
    (net (code "16") (name "unconnected-(U1-Pad5)")
      (node (ref "U1") (pin "5") (pinfunction "SDA") (pintype "bidirectional+no_connect")))
    (net (code "17") (name "unconnected-(U1-Pad6)")
      (node (ref "U1") (pin "6") (pinfunction "SCL") (pintype "bidirectional+no_connect")))
    (net (code "18") (name "unconnected-(U1-Pad7)")
      (node (ref "U1") (pin "7") (pinfunction "D4") (pintype "bidirectional+no_connect")))
    (net (code "19") (name "unconnected-(U1-Pad18)")
      (node (ref "U1") (pin "18") (pinfunction "F6") (pintype "bidirectional+no_connect")))
    (net (code "20") (name "unconnected-(U1-Pad19)")
      (node (ref "U1") (pin "19") (pinfunction "F5") (pintype "bidirectional+no_connect")))
    (net (code "21") (name "unconnected-(U1-Pad20)")
      (node (ref "U1") (pin "20") (pinfunction "F4") (pintype "bidirectional+no_connect")))
    (net (code "22") (name "unconnected-(U1-Pad22)")
      (node (ref "U1") (pin "22") (pinfunction "RST") (pintype "input+no_connect")))
    (net (code "23") (name "unconnected-(U1-Pad23)")
      (node (ref "U1") (pin "23") (pinfunction "GND") (pintype "power_in+no_connect")))
    (net (code "24") (name "unconnected-(U1-Pad24)")
      (node (ref "U1") (pin "24") (pinfunction "RAW") (pintype "power_out+no_connect")))))