(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001000_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers")
    )
  )

  (net 0 "")
  (net 1 "Net-(J2-Pad5)")
  (net 2 "Net-(J2-Pad4)")
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "unconnected-(U1-Pad1)")
  (net 7 "unconnected-(U1-Pad2)")
  (net 8 "unconnected-(U1-Pad3)")
  (net 9 "unconnected-(U1-Pad5)")
  (net 10 "unconnected-(U1-Pad6)")
  (net 11 "unconnected-(U1-Pad7)")
  (net 12 "unconnected-(U1-Pad18)")
  (net 13 "unconnected-(U1-Pad19)")
  (net 14 "unconnected-(U1-Pad20)")
  (net 15 "unconnected-(U1-Pad22)")
  (net 16 "unconnected-(U1-Pad23)")
  (net 17 "unconnected-(U1-Pad24)")
  (net 18 "Net-(U1-Pad13)")
  (net 19 "Net-(U1-Pad14)")
  (net 20 "Net-(U1-Pad15)")
  (net 21 "Net-(U1-Pad16)")
  (net 22 "Net-(U1-Pad17)")
  (net 23 "Net-(U1-Pad21)")
  (net 24 "Net-(U1-Pad4)")

  (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 623B7E9E) (tstamp 386a0090-0a46-4bfb-96d1-b3d435c60ba8)
    (at 123.2 76.5 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/8c077155-3d1b-4c61-8ad6-aa7da49ff67a")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.33 270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5ab39f29-a99d-4137-813c-0240aaa35e79)
    )
    (fp_text value "Conn_01x06" (at 0 -15.03 270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp e843b2f9-63bf-4162-9acd-99c55f41dac5)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 82e9af86-fd44-49c7-8996-479996b9b858)
    )
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp 28d92791-e03b-49b7-ab76-0b79e48b37f2))
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 2fe8fb82-a875-43d9-b72f-82742b7cdb00))
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 6c738b90-c565-4419-b3f8-c71fa068a959))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp a5860b45-4fc2-46a1-acd5-e3fbb8cba155))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp c8c88636-920e-4be2-a4e2-fc3f7ddd659c))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp e9ea7cf3-811f-4d45-affd-39be4058ac53))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 4a8a7ae8-e1f4-43bc-bf27-d27128fb055b))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 5dfe42c6-01b7-4abd-b9a5-6c91c2956ce9))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp d0a1fb4e-1977-4087-a971-99b683cf87ba))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp d4de041b-b58a-4daa-beee-c967a97f2743))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp 20afe9c7-7e63-485a-bab2-9fad3cd73f01))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 35cdb7da-6207-458e-b9a0-57079b9acb1f))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 41d14a77-a1a1-4f82-be40-67934bda1603))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp ba8befbb-68c6-431f-9d30-3f3bf9a6b7e3))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp c9ad0256-e795-473a-9d31-5442242d3188))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad21)") (pinfunction "Pin_1") (pintype "passive") (tstamp 18c97c17-4686-4762-ac2f-547b5b999ca9))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad17)") (pinfunction "Pin_2") (pintype "passive") (tstamp 519527ee-f2dc-482d-94bb-75721ed8aafb))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad16)") (pinfunction "Pin_3") (pintype "passive") (tstamp c7878c4f-2f8a-4bbb-adbc-833e5b6f7423))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad15)") (pinfunction "Pin_4") (pintype "passive") (tstamp 5ca1b4f0-e4cd-4f1a-9bfa-ba57d20cfd00))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad14)") (pinfunction "Pin_5") (pintype "passive") (tstamp 8f6e74de-71c3-4969-bfa3-21ee2db29d12))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad13)") (pinfunction "Pin_6") (pintype "passive") (tstamp 56486356-64f4-4148-b335-6b45c342341d))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Creadas:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 623B7ECA) (tstamp 7783caad-32e1-4cb9-a1e2-e38997af04a8)
    (at 182.375 76.475 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/abc425ae-34db-440c-baf2-199506429483")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.33 270) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cc4f0b33-ccfd-419b-9659-a88488fda9d5)
    )
    (fp_text value "Conn_01x06" (at 0 -15.03 270) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c93092f3-ad93-4616-a7d6-461e3ba02b31)
    )
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4770ef60-21bb-4d72-93b1-855cef6e8fb9)
    )
    (fp_line (start -1.33 -1.27) (end -1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp 209b39ed-1521-46f3-985b-6f682af8a636))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer "B.SilkS") (width 0.12) (tstamp 23b01e04-7511-4c52-80ed-871675300ee9))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer "B.SilkS") (width 0.12) (tstamp 42f5b5b4-dd5c-4778-98da-3fe6b6b36b6c))
    (fp_line (start 1.33 -1.27) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp a001f9b3-d55c-45e5-82b3-54c3c57f50f4))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer "B.SilkS") (width 0.12) (tstamp a12176d4-cccd-4936-bd41-2b7cdce20b70))
    (fp_line (start -1.33 -14.03) (end 1.33 -14.03) (layer "B.SilkS") (width 0.12) (tstamp d5ed5e46-d54a-447d-9f4b-f0768c1fbc9a))
    (fp_line (start -1.8 1.8) (end -1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 0fb612b6-d118-463f-8273-72d16ac7c8f3))
    (fp_line (start -1.8 -14.5) (end 1.8 -14.5) (layer "B.CrtYd") (width 0.05) (tstamp 3825ef5a-9c20-4da1-b237-0d7cce88677d))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp 524dfc74-a6ca-4f47-b1c4-8c830a3897c9))
    (fp_line (start 1.8 -14.5) (end 1.8 1.8) (layer "B.CrtYd") (width 0.05) (tstamp cef8d6fd-fad1-4b1e-bfe8-44b8b9fd4ec5))
    (fp_line (start -1.27 -13.97) (end -1.27 0.635) (layer "B.Fab") (width 0.1) (tstamp 207c4811-314a-47bb-ae18-2f9379831b81))
    (fp_line (start 1.27 -13.97) (end -1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 241d45c3-e292-4286-88e2-648d09936352))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer "B.Fab") (width 0.1) (tstamp 543ccabc-4148-495e-bbf3-b3f2d2fb3d9e))
    (fp_line (start 1.27 1.27) (end 1.27 -13.97) (layer "B.Fab") (width 0.1) (tstamp 789fde59-6346-41c4-8bdd-f9aa5fd7f3db))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer "B.Fab") (width 0.1) (tstamp 89e85ee3-bf08-4d94-97ac-77b0e3f043c9))
    (pad "1" thru_hole rect (at 0 0 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 2ff20828-bd59-4b9f-96ee-57d97ba845ab))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 756c320d-1757-4c24-8d25-eea4479fc01c))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp 35301f71-3327-4814-addd-6803f155857b))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp dddee525-5a91-4e7c-9753-319ed47ddcc0))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 008d03ef-d971-462c-bfb3-7aa302eab0fd))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 3 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad4)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7ac680eb-02c3-488d-9052-a4bda05e99dd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "M:/pin-headers-1.snapshot.5/Pin Header 1x6 TH Pitch 2.54mm.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Creadas:ProMicro" (layer "B.Cu")
    (tedit 623B8046) (tstamp c1b78138-c11c-4fb6-bc53-1e102c698b86)
    (at 145 89.77 -90)
    (descr "Pro Micro footprint")
    (tags "promicro ProMicro")
    (property "Sheetfile" "numPAD_MCU.kicad_sch")
    (property "Sheetname" "")
    (path "/c71f56c1-5b7c-4373-9716-fffac482104c")
    (attr through_hole)
    (fp_text reference "U1" (at 0 10.16 90) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2135eddd-f41f-4ab2-a263-8dadf6425926)
    )
    (fp_text value "ProMicro" (at 0 -10.16 90) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 642c3167-61ff-412b-b7c2-23be8f7d6d81)
    )
    (fp_line (start -15.24 -8.89) (end 15.24 -8.89) (layer "B.SilkS") (width 0.15) (tstamp 02b95530-09eb-4a8e-a488-67c549fc95da))
    (fp_line (start -15.24 8.89) (end 15.24 8.89) (layer "B.SilkS") (width 0.15) (tstamp 1cd8e2a0-99d1-450c-aa49-c54d9399ba6b))
    (fp_line (start -15.24 -8.89) (end -15.24 -3.81) (layer "B.SilkS") (width 0.15) (tstamp 3e368736-42ee-49e8-b8e6-92f23d085d37))
    (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer "B.SilkS") (width 0.15) (tstamp aed1af86-2fd4-47a3-a678-1eaf5b9cda50))
    (fp_line (start -17.78 -3.81) (end -17.78 3.81) (layer "B.SilkS") (width 0.15) (tstamp b82d984a-2a78-4dbf-9516-5c16648505e3))
    (fp_line (start -15.24 -3.81) (end -17.78 -3.81) (layer "B.SilkS") (width 0.15) (tstamp deca1926-78fc-4dc2-8b2d-b454284b8ba9))
    (fp_line (start -15.24 3.81) (end -15.24 8.89) (layer "B.SilkS") (width 0.15) (tstamp e190aa7b-5147-4d85-8d47-de2af4e5add9))
    (fp_line (start -17.78 3.81) (end -15.24 3.81) (layer "B.SilkS") (width 0.15) (tstamp f195d16d-ee5a-46c9-bfed-922f99074f3e))
    (pad "1" thru_hole rect (at -13.97 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 6 "unconnected-(U1-Pad1)") (pinfunction "TX") (pintype "bidirectional+no_connect") (tstamp 20ded32e-6cec-4642-9bbf-bec8a4313054))
    (pad "2" thru_hole oval (at -11.43 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 7 "unconnected-(U1-Pad2)") (pinfunction "RX") (pintype "bidirectional+no_connect") (tstamp e444c522-353b-4c32-a29c-27f7d80eb8d7))
    (pad "3" thru_hole oval (at -8.89 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 8 "unconnected-(U1-Pad3)") (pinfunction "GND") (pintype "power_in+no_connect") (tstamp db3b5812-159f-4218-aac7-75d053a4d199))
    (pad "4" thru_hole oval (at -6.35 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 24 "Net-(U1-Pad4)") (pinfunction "GND") (pintype "power_in") (tstamp 830d8dfa-69fa-4cf9-8d51-65cceb582110))
    (pad "5" thru_hole oval (at -3.81 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 9 "unconnected-(U1-Pad5)") (pinfunction "SDA") (pintype "bidirectional+no_connect") (tstamp 89061b42-bdae-4630-82ba-272670b4f27d))
    (pad "6" thru_hole oval (at -1.27 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 10 "unconnected-(U1-Pad6)") (pinfunction "SCL") (pintype "bidirectional+no_connect") (tstamp 14816cdb-f803-40c8-89cf-68b16fa15c10))
    (pad "7" thru_hole oval (at 1.27 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 11 "unconnected-(U1-Pad7)") (pinfunction "D4") (pintype "bidirectional+no_connect") (tstamp 48e5b7a6-0e4d-4865-a203-7b9471d025f7))
    (pad "8" thru_hole oval (at 3.81 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 1 "Net-(J2-Pad5)") (pinfunction "C6") (pintype "bidirectional") (tstamp ad40c983-f57f-4b8e-a3bf-b2b9aacd6fea))
    (pad "9" thru_hole oval (at 6.35 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 2 "Net-(J2-Pad4)") (pinfunction "D7") (pintype "bidirectional") (tstamp a66818c8-2ced-42b9-b3bf-b5a68a2926fb))
    (pad "10" thru_hole oval (at 8.89 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 3 "Net-(J2-Pad3)") (pinfunction "E6") (pintype "bidirectional") (tstamp 0afa9efe-7d2f-4a19-99dd-8dcd3edb1ab5))
    (pad "11" thru_hole oval (at 11.43 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 4 "Net-(J2-Pad2)") (pinfunction "B4") (pintype "bidirectional") (tstamp b400ebaf-6b57-44f1-9567-307212111260))
    (pad "12" thru_hole oval (at 13.97 -7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 5 "Net-(J2-Pad1)") (pinfunction "B5") (pintype "bidirectional") (tstamp 51fb00d7-24f9-4376-8d7b-c05ca25bcc28))
    (pad "13" thru_hole oval (at 13.97 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 18 "Net-(U1-Pad13)") (pinfunction "B6") (pintype "bidirectional") (tstamp 9bb640fc-fb87-47c3-ac83-b57dadd051cb))
    (pad "14" thru_hole oval (at 11.43 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 19 "Net-(U1-Pad14)") (pinfunction "B2") (pintype "bidirectional") (tstamp cbedae76-c5ff-4803-b4b9-c87aabd0a33f))
    (pad "15" thru_hole oval (at 8.89 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 20 "Net-(U1-Pad15)") (pinfunction "B3") (pintype "bidirectional") (tstamp 218f9185-7f56-42e5-8e76-84479290cb98))
    (pad "16" thru_hole oval (at 6.35 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 21 "Net-(U1-Pad16)") (pinfunction "B1") (pintype "bidirectional") (tstamp faa7310e-7d63-48e4-99eb-3069816753f0))
    (pad "17" thru_hole oval (at 3.81 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 22 "Net-(U1-Pad17)") (pinfunction "F7") (pintype "bidirectional") (tstamp d7328f0a-9d1b-4ed4-b09d-d92654faf8d8))
    (pad "18" thru_hole oval (at 1.27 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 12 "unconnected-(U1-Pad18)") (pinfunction "F6") (pintype "bidirectional+no_connect") (tstamp 0b3390cd-74f6-475b-9859-e721e89b07bd))
    (pad "19" thru_hole oval (at -1.27 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 13 "unconnected-(U1-Pad19)") (pinfunction "F5") (pintype "bidirectional+no_connect") (tstamp 82e16a6a-b2c8-4127-b702-a933d49a8632))
    (pad "20" thru_hole oval (at -3.81 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 14 "unconnected-(U1-Pad20)") (pinfunction "F4") (pintype "bidirectional+no_connect") (tstamp 283bb057-fadb-4943-99d0-ab38c6ed1303))
    (pad "21" thru_hole oval (at -6.35 7.62 270) (size 1.62 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 23 "Net-(U1-Pad21)") (pinfunction "VCC") (pintype "power_in") (tstamp 0d9713e7-b681-43f3-9e01-3339694f481d))
    (pad "22" thru_hole oval (at -8.89 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 15 "unconnected-(U1-Pad22)") (pinfunction "RST") (pintype "input+no_connect") (tstamp 331fc480-04a0-4bda-9dbb-20beb121452b))
    (pad "23" thru_hole oval (at -11.43 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 16 "unconnected-(U1-Pad23)") (pinfunction "GND") (pintype "power_in+no_connect") (tstamp 965c2489-f33d-47e8-9298-5a61e3c0971a))
    (pad "24" thru_hole oval (at -13.97 7.62 270) (size 2 3) (drill 1.1) (layers *.Cu "F.Mask")
      (net 17 "unconnected-(U1-Pad24)") (pinfunction "RAW") (pintype "power_out+no_connect") (tstamp f66f9e8b-42f3-4267-b9bc-9a5e3781d428))
    (model "M:/ARDUINO PRO MICRO.STEP"
      (offset (xyz -13.95 -7.65 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (gr_line (start 108 105.5) (end 185 105.5) (layer "Edge.Cuts") (width 0.1) (tstamp 10c879d5-cd08-480e-8102-309b8ecea393))
  (gr_line (start 108 74.5) (end 185 74.5) (layer "Edge.Cuts") (width 0.15) (tstamp 7c55386f-d887-4962-bb89-7e762c57040b))
  (gr_line (start 108 74.5) (end 108 105.5) (layer "Edge.Cuts") (width 0.1) (tstamp 96e75cf1-87d1-4b52-b945-bcd73be8c263))
  (gr_line (start 185 74.5) (end 185 105.5) (layer "Edge.Cuts") (width 0.1) (tstamp fe651e19-573a-4fda-9b07-e9e295dc239b))
  (dimension (type aligned) (layer "Eco2.User") (tstamp cac811e8-03ed-4488-8c79-595617da12c8)
    (pts (xy 185 74.5) (xy 108 74.5))
    (height 3.5)
    (gr_text "77,0000 mm" (at 146.5 69.85) (layer "Eco2.User") (tstamp cac811e8-03ed-4488-8c79-595617da12c8)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Eco2.User") (tstamp fa622127-2c8b-45a5-b225-aeabe299c2e5)
    (pts (xy 108 74.5) (xy 108 105.5))
    (height 4)
    (gr_text "31,0000 mm" (at 102.85 90 90) (layer "Eco2.User") (tstamp a49a89e5-63b0-4848-88da-c2ac2750bedf)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 166.42 93.58) (end 152.62 93.58) (width 1) (layer "F.Cu") (net 1) (tstamp 59b8acca-a31d-4968-8a25-01bf543ffede))
  (segment (start 172.215 76.475) (end 172.215 87.785) (width 1) (layer "F.Cu") (net 1) (tstamp 74d44543-bc28-457d-8af1-84d57056a44a))
  (segment (start 172.215 87.785) (end 166.42 93.58) (width 1) (layer "F.Cu") (net 1) (tstamp e85ae780-6638-4d64-8333-4b09a83267db))
  (segment (start 174.755 91.245) (end 169.88 96.12) (width 1) (layer "F.Cu") (net 2) (tstamp 0391a3d3-c63b-4138-9835-a57ac2ce5fc1))
  (segment (start 174.755 76.475) (end 174.755 91.245) (width 1) (layer "F.Cu") (net 2) (tstamp 7abe10cf-a81f-4fe4-bb88-bbbe240ecb03))
  (segment (start 169.88 96.12) (end 152.62 96.12) (width 1) (layer "F.Cu") (net 2) (tstamp bd18cc6c-c395-4302-85c3-eb26db03ddfe))
  (segment (start 177.295 94.205) (end 172.84 98.66) (width 1) (layer "F.Cu") (net 3) (tstamp 301f05d3-4eeb-4769-b5a1-37ff99c8342b))
  (segment (start 177.295 76.475) (end 177.295 94.205) (width 1) (layer "F.Cu") (net 3) (tstamp 3f352e94-7ad2-41ca-bf3b-e46e0ae766cd))
  (segment (start 172.84 98.66) (end 152.62 98.66) (width 1) (layer "F.Cu") (net 3) (tstamp 5b44dddd-fc3a-475c-a08c-e6a8622d4886))
  (segment (start 179.835 96.665) (end 175.3 101.2) (width 1) (layer "F.Cu") (net 4) (tstamp 1bba85b3-e8a4-4045-9fef-8ead3577213c))
  (segment (start 179.835 76.475) (end 179.835 96.665) (width 1) (layer "F.Cu") (net 4) (tstamp 5d1b609c-ab4a-420a-a3bd-0dffa564c964))
  (segment (start 175.3 101.2) (end 152.62 101.2) (width 1) (layer "F.Cu") (net 4) (tstamp 9b73e8bf-9768-4e4b-9a25-6b946fc2ad66))
  (segment (start 178.76 103.74) (end 152.62 103.74) (width 1) (layer "F.Cu") (net 5) (tstamp 4447713b-4b09-4ef6-a20f-5a2b8a2e2fe8))
  (segment (start 182.375 76.475) (end 182.375 100.125) (width 1) (layer "F.Cu") (net 5) (tstamp 46dce890-3c9a-4ee9-b7bc-857e7fb8322d))
  (segment (start 182.375 100.125) (end 178.76 103.74) (width 1) (layer "F.Cu") (net 5) (tstamp cd8d6ee2-52fc-406c-9b9e-4bef693c8c31))
  (segment (start 110.5 76.5) (end 110.5 95) (width 1) (layer "F.Cu") (net 18) (tstamp a5f44437-4ba2-454c-b434-6854351bc562))
  (segment (start 119.24 103.74) (end 137.38 103.74) (width 1) (layer "F.Cu") (net 18) (tstamp c9f106ed-ef89-456b-a7d8-632de2b42633))
  (segment (start 110.5 95) (end 119.24 103.74) (width 1) (layer "F.Cu") (net 18) (tstamp d0095a70-c0ad-46af-a915-097d5eea7fb4))
  (segment (start 113.04 90.46) (end 113 90.5) (width 1) (layer "F.Cu") (net 19) (tstamp 5368a802-6a1e-416a-afe4-ffd4b990037f))
  (segment (start 113 93.5) (end 120.7 101.2) (width 1) (layer "F.Cu") (net 19) (tstamp 93c963af-9a42-4352-9207-6023a3c0743c))
  (segment (start 113.04 76.5) (end 113.04 90.46) (width 1) (layer "F.Cu") (net 19) (tstamp a08bdc80-a064-4918-a7c8-07fd0f1ad1ad))
  (segment (start 113 90.5) (end 113 93.5) (width 1) (layer "F.Cu") (net 19) (tstamp a0bf9a64-3c5e-43fa-9c51-b33162c91d70))
  (segment (start 120.7 101.2) (end 137.38 101.2) (width 1) (layer "F.Cu") (net 19) (tstamp c0b1c111-0e6d-4508-b051-ad7ac968c3be))
  (segment (start 122.66 98.66) (end 137.38 98.66) (width 1) (layer "F.Cu") (net 20) (tstamp 36722f55-e96e-466f-99f9-7a01796aef32))
  (segment (start 115.58 76.5) (end 115.58 91.58) (width 1) (layer "F.Cu") (net 20) (tstamp 515b8baf-9017-4443-8003-b389e6ce96d2))
  (segment (start 115.58 91.58) (end 122.66 98.66) (width 1) (layer "F.Cu") (net 20) (tstamp b967be99-b116-4136-8ef7-5e6d4f363c0d))
  (segment (start 118.12 89.12) (end 125.12 96.12) (width 1) (layer "F.Cu") (net 21) (tstamp 5a4c00e2-f42c-4c02-8da5-cdb8f7e08f84))
  (segment (start 118.12 76.5) (end 118.12 89.12) (width 1) (layer "F.Cu") (net 21) (tstamp 74f9f0f2-e076-4404-afc6-72cf00822153))
  (segment (start 125.12 96.12) (end 137.38 96.12) (width 1) (layer "F.Cu") (net 21) (tstamp ea8e6c00-9813-4e5e-aa09-c68436925ffe))
  (segment (start 126.58 93.58) (end 137.38 93.58) (width 1) (layer "F.Cu") (net 22) (tstamp 4788817c-7fac-448b-ab23-13dfed734205))
  (segment (start 120.66 76.5) (end 120.66 87.66) (width 1) (layer "F.Cu") (net 22) (tstamp 7493c0ca-206c-4751-b3cf-b40e0dc8052d))
  (segment (start 120.66 87.66) (end 126.58 93.58) (width 1) (layer "F.Cu") (net 22) (tstamp 846b9d2b-fa57-4250-8ed4-3287ef873c1b))
  (segment (start 123.2 80.2) (end 126.42 83.42) (width 1) (layer "F.Cu") (net 23) (tstamp 461af355-6f5a-4f9c-96a9-f13d6d323d30))
  (segment (start 126.42 83.42) (end 137.38 83.42) (width 1) (layer "F.Cu") (net 23) (tstamp 51ce7c21-6e68-4bb3-97f5-7bdb38cf5641))
  (segment (start 123.2 76.5) (end 123.2 80.2) (width 1) (layer "F.Cu") (net 23) (tstamp bfd61fee-07f9-4793-9681-b9d8ebf1413c))
  (segment (start 169.675 76.475) (end 169.675 80.325) (width 1) (layer "F.Cu") (net 24) (tstamp 67dccf47-edb2-41b5-8101-a4f321faf68a))
  (segment (start 169.675 80.325) (end 166.58 83.42) (width 1) (layer "F.Cu") (net 24) (tstamp 832faf4d-3bbe-48b0-b081-92cefd3c4e42))
  (segment (start 166.58 83.42) (end 152.62 83.42) (width 1) (layer "F.Cu") (net 24) (tstamp c7afd03a-61b0-4148-a40c-8b8310172323))

)
